# Getting Started

Getting Started

## Finding a location for your photo printer

## Finding a location for your printer

* Place the photo printer on a flat, clean and dust-free surface, **in a dry location**, and *out of direct sunlight*.

Note:

* For proper ventilation[[1]](#footnote-1), make sure the top and back of the photo printer are not blocked.

## Connecting and turning on the power

Turning on the power

Note: Use only the AC power adapter included with your photo printer. Other adapters can damage your camera, photo printer, or computer.



To connect and turn on the power, follow these steps:

|  |  |
| --- | --- |
| **Step** | **Notes** |
| 1. Connect the AC power cord to the AC power adapter, then to the back of the photo printer. | The AC power cable included with your photo printer may not require assembly, and may be different from the one shown. |
| 1. Plug the AC power cable into a power outlet. |  |
| 1. Press the On / Off button to turn the power on. | The photo printer initializes and the On/Off button glows steady green. |

1. Allow enough space on all sides of the photo printer to let you connect and disconnect cables, change the color cartridge, and add paper. [↑](#footnote-ref-1)